Programmable interrupt controller ignores keystrike.

If we want to get it, we have to tell to pic to not to ignore it.

outb assembly instruction takes 2 parameters: port number and data you want to send.

We will create 2 more files:

* port.h
* port.cpp